**604 Crate Late Models**  
SPEC Tires only FT200, FT400, HTS 1350, HTS 1600, Crate 21 or Crate 55, American Racer spec 48 & spec 56. Samples will be taken - Grooving and siping are allowed.

All spoilers are 8" and 8" sides. Deck is 39" no tolerance.

All other Rules: Nesmith, Fastrak and SECA 2017 are allowed.

Weight 2300 lbs. One pound per lap burn-off in A-Main only. All other times must weigh 2300lbs.